Windowed Watchdog Timer (WWDT) Example
======================================

Example description
The WWDT example demonstrates the handling of WDT warning trigger interrupt
to enable "safe" operation. The watchdog generates a warning WWDT interrupt
and then feeds the WWDT on the warning. The LED0 will toggle on each warning
interval cycle.

Special connection requirements
-------------------------------
Board [NXP_LPCXPRESSO_812]:
There are no special connection requirements for this example.

Board [NXP_812_MAX]:
There are no special connection requirements for this example.

Board [NXP_LPCXPRESSO_824]:
There are no special connection requirements for this example.

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.
