UART API in ROM (USART API ROM) Polling Example
===============================================

Example Description
-------------------
The UART_ROM example demonstrates using the USART API ROM functions
in polling mode for terminated data input and output and single byte
input and output.

Special connection requirements
-------------------------------
Board [NXP_LPCXPRESSO_812]:
See @ref LPCOPEN_8XX_BOARD_LPCXPRESSO_812 for information on how to
setup the UART port hardware with this example..

Board [NXP_812_MAX]:
See LPC812_max-UART.txt for UART configuration details.

Board [NXP_LPCXPRESSO_824]:
See LPC824_xpresso-UART.txt for UART configuration details.

Build procedures:
Visit the <a href="http://www.lpcware.com/content/project/lpcopen-platform-nxp-lpc-microcontrollers/lpcopen-v200-quickstart-guides">LPCOpen quickstart guides</a>
to get started building LPCOpen projects.
